Nokia N800 and N810 tablets (n800, n810) — QEMU 5.1.0 (v5.1.0-11824-g8699890d91-dirty) documentation

# Nokia N800 and N810 tablets (`n800`, `n810`)

Nokia N800 and N810 internet tablets (known also as RX-34 and RX-44 / 48) emulation supports the following elements:

- Texas Instruments OMAP2420 System-on-chip (ARM1136 core)

- RAM and non-volatile OneNAND Flash memories

- Display connected to EPSON remote framebuffer chip and OMAP on-chip display controller and a LS041y3 MIPI DBI-C controller

- TI TSC2301 (in N800) and TI TSC2005 (in N810) touchscreen controllers driven through SPI bus

- National Semiconductor LM8323-controlled qwerty keyboard driven through I2C bus

- Secure Digital card connected to OMAP MMC/SD host

- Three OMAP on-chip UARTs and on-chip STI debugging console

- Mentor Graphics “Inventra” dual-role USB controller embedded in a TI TUSB6010 chip - only USB host mode is supported

- TI TMP105 temperature sensor driven through I2C bus

- TI TWL92230C power management companion with an RTC on I2C bus

- Nokia RETU and TAHVO multi-purpose chips with an RTC, connected through CBUS