Arm Versatile boards (versatileab, versatilepb) — QEMU 5.1.0 (v5.1.0-11824-g8699890d91-dirty) documentation

# Arm Versatile boards (`versatileab`, `versatilepb`)

The Arm Versatile baseboard is emulated with the following devices:

- ARM926E, ARM1136 or Cortex-A8 CPU

- PL190 Vectored Interrupt Controller

- Four PL011 UARTs

- SMC 91c111 Ethernet adapter

- PL110 LCD controller

- PL050 KMI with PS/2 keyboard and mouse.

- PCI host bridge. Note the emulated PCI bridge only provides access to PCI memory space. It does not provide access to PCI IO space. This means some devices (eg. ne2k_pci NIC) are not usable, and others (eg. rtl8139 NIC) are only usable when the guest drivers use the memory mapped control registers.

- PCI OHCI USB controller.

- LSI53C895A PCI SCSI Host Bus Adapter with hard disk and CD-ROM devices.

- PL181 MultiMedia Card Interface with SD card.