Sharp XScale-based PDA models (akita, borzoi, spitz, terrier) — QEMU 5.1.0 (v5.1.0-11824-g8699890d91-dirty) documentation

# Sharp XScale-based PDA models (`akita`, `borzoi`, `spitz`, `terrier`)

The XScale-based clamshell PDA models (“Spitz”, “Akita”, “Borzoi” and “Terrier”) emulation includes the following peripherals:

- Intel PXA270 System-on-chip (ARMv5TE core)

- NAND Flash memory

- IBM/Hitachi DSCM microdrive in a PXA PCMCIA slot - not in “Akita”

- On-chip OHCI USB controller

- On-chip LCD controller

- On-chip Real Time Clock

- TI ADS7846 touchscreen controller on SSP bus

- Maxim MAX1111 analog-digital converter on I2C bus

- GPIO-connected keyboard controller and LEDs

- Secure Digital card connected to PXA MMC/SD host

- Three on-chip UARTs

- WM8750 audio CODEC on I2C and I2S busses