ColdFire System emulator — QEMU 5.1.0 (v5.1.0-11824-g8699890d91-dirty) documentation

# ColdFire System emulator

Use the executable `qemu-system-m68k` to simulate a ColdFire machine. The emulator is able to boot a uClinux kernel.

The M5208EVB emulation includes the following devices:

- MCF5208 ColdFire V2 Microprocessor (ISA A+ with EMAC).

- Three Two on-chip UARTs.

- Fast Ethernet Controller (FEC)

The AN5206 emulation includes the following devices:

- MCF5206 ColdFire V2 Microprocessor.

- Two on-chip UARTs.